1.> Netwrok topology:

PC(D-view6)10.90.90.200---(P1/1)DES7200,10.90.90.90

2.> DES-7200 configuration:

interface VLAN 1

ip address 10.90.90.90 255.0.0.0

snmp-server community public RO


snmp-server community private RW

snmp-server enable traps


snmp-server host 10.90.90.200 public

3.> D-View6 setting

a.> Use Setup Wizard




b.> Click Next




c.> Give a Domain name ‘**test**’

Click ‘***Create***’

Click ‘***Next***’




d.> Enter a name of NETMAP, click ***Next***




e.> Choose **Designated Network**

Give a name of Topology


Click **Next**



f.> Issue switch’s information & SNMP community string. Click Finish



g.> Click Export



h.> Double click Net-10.0.0.0

Double click the DES7200’s icon

Select Private Mib-> CPU Utilization

