How to setup L2TP over IPsec on the DFL-series

Topology:

   

 L2TP over IPsec Server L2TP over IPsec user

1. Add 2 address object “l2tp-server” and “l2tp-pool”.



1. Add a new pre-share key.



1. Add a new IPsec interface.

Local network “wan-IP”

Remote network “all-nets”

Mode “transport”









1. Add a new LTP server interface.

Inner IP address: “L2TP-server”

Tunnel protocol: “L2TP”

Outer interface: “IPsec-RA”

Server IP: “WAN\_IP”







(5)

Add a new interface group for “L2TP-interface” and “LAN”.



1. Add a new IP rule for L2TP user.



1. Add new L2TP user account.







 END