
**How to manage AP on DWS-3160 over IPsec?**


****Step 1. Set up DWS-6600 IP to be 192.168.10.2/24


Step 2. Set up DWR-250A IP configuration



Step 3. Go to DWS-205A VPN Setting->IPset->IPsec policies.


Set up DWR-250A IPsec configuration.



Step 4. Set up DWR-250B IP configuration  



Step 5. Go to DWS-205B VPN Setting->IPsec->IPsec policies.

Set up DWR-250B IPsec configuration.




Step 6. Set up DWS-4026 L3 Interface.


For Port 13.




For Port 14.




Step 7. Establish IPsec connection between DSR-A and DSR-B




Check Link status




Step 8. Set up DWS-3160 IP configuration



Step 9. Enable L3/IP Discovery and add AP’s IP address 192.168.10.2.



Step 10. Go to mentoring->Access Point->All AP status and then manage AP



Result：D:\Setting\Desktop\Untitled.png