
How to setup PPTP ALG

Topology:

IP: 192.168.1.10/24


LAN: 192.168.1.1/24

 DFL-860E: PPTP server

WAN1: static ip



WAN: PPPoE

 DFL-260E: PPTP ALG

LAN:192.168.10.1/24


 IP: 192.168.10.10/24

PPTP client


You can study “NetDefendOS\_2.27.03\_Firewall\_UserManual” P.269 chapter 6.2.7. “The PPTP ALG”. It can make you understand PPTP ALG more detail.


DFL-260E

(1)Go to “ALG with AV/WCF”. Add a new ALG “PPTP-ALG”.




(2) Go to “Service”. Add a new “PPTP-service”.







(3)Go to “IP Rules”. Add a new “PPTP” rule.




(4)






DFL-860E


(1) Go to “Address book”. Add two new IP objects.




(2) Go to “PPTP server”.




(3) Go to “AdminUsers”. Add a new user “dlink”.



(4) Go to “User Authentication Rules”. Add a new rule “PPTP”.





(5)Go to “IP Rules”. Add a new “PPTP” rule.

