
How to setup SSL VPN on DFL

Topology:


PC 1 -------------------------- DFL (PPPoE) -------------Internet------------SSL client

Setup:

1. Check firmware. You need to use 2.30.01.06.




1. Add a new PPPoE interface.




1. Add a new SSL VPN interface. Inter IP and IP address pool must be in the same subnet.


Outer interface: PPPoE

Server IP: pppoe\_ip




**Note:**





About more SSL VPN information, please read “NetDefendOS\_2.40.00\_Firewall\_UserManual”.

1. Add a new SSL VPN user “dlink”.





1. Go to “User Authentication rules”.

Interface: SSL-VPN


Originator IP: all-nets

Terminator IP: PPPOE\_ip





1. Add 2 IP rules for SSL VPN user.



1. You can use SSL VPN client to connect DFL.

END