DFL-Routing Mode

Topology



ISP: 192.168.0.0/24


WAN1 IP: 192.168.0.10/24




LAN IP: 1.1.1.1/24

 IP: 1.1.1.10/24


1. Change your firewall DNS IP address.




1. Setup WAN1\_IP. Do not use “default gateway”.





(3)Do not choose these two buttons.




(4)Setup LAN\_IP.









(5)Creating two new routing.




(6)Change IP rules. All IP rules are use “allow” and I create a new rule “all-service” for tested.



(7)Create a new IP rule for WAN1 to LAN1.



(8)Save configuration.



End