How to setup SIP ALG

  SIP Server: Public IP

 Internet

 WAN IP: PPPoE

 DFL-800

  

 SIP Phone: X-Lite 4.0 SIP Phone: X-Lite 4.0

This topology is reference “NetDefendOS\_2.27.03\_Firewall\_UserManual” P.273 scenario 1. You can study chapter 6.2.8. “The SIP ALG”. It can make you understand SIP ALG more detail.

1. Add a new SIP ALG.



1. Add a new SIP-UDP service.





1. Add two new IP rules “SIP” and “SIP-IN”.



1. Change timeout settings.

