How to setup SSL VPN on DFL

Topology:

PC 1 -------------------------- DFL (PPPoE) -------------Internet------------SSL client

Setup:

1. Check firmware. You need to use 2.30.01.06.



1. Add a new PPPoE interface.



1. Add a new SSL VPN interface. Inter IP and IP address pool must be in the same subnet.

Outer interface: PPPoE

Server IP: pppoe\_ip



**Note:**





About more SSL VPN information, please read “NetDefendOS\_2.40.00\_Firewall\_UserManual”.

1. Add a new SSL VPN user “dlink”.



1. Go to “User Authentication rules”.

Interface: SSL-VPN

Originator IP: all-nets

Terminator IP: PPPOE\_ip





1. Add 2 IP rules for SSL VPN user.



1. You can use SSL VPN client to connect DFL.

 END