**[Topology]**PC(10.90.90.100)----(1/1)DES-7200

**[Configuration]**!
username test password test
username test privilege 15
ip http authentication local
!
enable service web-server http
enable service web-server https
!
interface VLAN 1
 no ip proxy-arp
 ip address 10.90.90.90 255.0.0.0
!

Then, open the browser with <http://10.90.90.90> with **user name: test, password: test.**