DFL-Routing Mode

Topology

 

 ISP: 192.168.0.0/24

 WAN1 IP: 192.168.0.10/24

 

 LAN IP: 1.1.1.1/24

  IP: 1.1.1.10/24

1. Change your firewall DNS IP address.



1. Setup WAN1\_IP. Do not use “default gateway”.



(3)Do not choose these two buttons.



(4)Setup LAN\_IP.







(5)Creating two new routing.



(6)Change IP rules. All IP rules are use “allow” and I create a new rule “all-service” for tested.



(7)Create a new IP rule for WAN1 to LAN1.



(8)Save configuration.



End