**[Topology]**PC(10.90.90.100)----(1/1)DES-7200

**[Configuration]**!  
username test password test  
username test privilege 15  
ip http authentication local  
!  
enable service web-server http  
enable service web-server https  
!  
interface VLAN 1  
 no ip proxy-arp  
 ip address 10.90.90.90 255.0.0.0  
!

Then, open the browser with <http://10.90.90.90> with **user name: test, password: test.**