
**DHP-306AV/DHP-307AV firmware upgrade utility guide**

**System requirements**

**Windows XP,** **Windows Vista, or Windows 7** with network support.

**Step 1: Install the utility**


Follow the wizard’s instructions to install the firmware upgrade utility.




**Step 2: Connect to device**

Plug the DHP-306AV into an AC wall outlet. Connect one end of the supplied CAT5 Ethernet cable to the Ethernet port of the DHP-306AV and the other end of the cable to the Ethernet port of your computer.

**Step 3: Run the utility**


Follow these simple steps to upgrade your device. 

Note: Do not turn off the power and disconnect the Ethernet cable before the process has completed.



**Step 4: Upgrade completed**

When the firmware upgrade process has completed, the following screenshot will be displayed. If the update was not successful, please run the utility again.



Note: For DHP-307AV users, please connect to another one DHP-306AV first and then go back to Step 2.